SNMPv2-SMI DEFINITIONS ::= BEGIN

-- the path to the root

org            OBJECT IDENTIFIER ::= { iso 3 }  --  "iso" = 1
dod            OBJECT IDENTIFIER ::= { org 6 }
internet       OBJECT IDENTIFIER ::= { dod 1 }

directory      OBJECT IDENTIFIER ::= { internet 1 }

mgmt           OBJECT IDENTIFIER ::= { internet 2 }
mib-2          OBJECT IDENTIFIER ::= { mgmt 1 }
transmission   OBJECT IDENTIFIER ::= { mib-2 10 }

experimental   OBJECT IDENTIFIER ::= { internet 3 }

private        OBJECT IDENTIFIER ::= { internet 4 }
enterprises    OBJECT IDENTIFIER ::= { private 1 }

security       OBJECT IDENTIFIER ::= { internet 5 }

snmpV2         OBJECT IDENTIFIER ::= { internet 6 }

-- transport domains
snmpDomains    OBJECT IDENTIFIER ::= { snmpV2 1 }

-- transport proxies
snmpProxys     OBJECT IDENTIFIER ::= { snmpV2 2 }

-- module identities
snmpModules    OBJECT IDENTIFIER ::= { snmpV2 3 }

-- Extended UTCTime, to allow dates with four-digit years
-- (Note that this definition of ExtUTCTime is not to be IMPORTed
--  by MIB modules.)
ExtUTCTime ::= OCTET STRING(SIZE(11 | 13))
    -- format is YYMMDDHHMMZ or YYYYMMDDHHMMZ

    --   where: YY   - last two digits of year (only years
    --                 between 1900-1999)
    --          YYYY - last four digits of the year (any year)
    --          MM   - month (01 through 12)
    --          DD   - day of month (01 through 31)
    --          HH   - hours (00 through 23)
    --          MM   - minutes (00 through 59)
    --          Z    - denotes GMT (the ASCII character Z)
    --
    -- For example, "9502192015Z" and "199502192015Z" represent
    -- 8:15pm GMT on 19 February 1995. Years after 1999 must use
    -- the four digit year format. Years 1900-1999 may use the
    -- two or four digit format.

-- definitions for information modules

MODULE-IDENTITY MACRO ::=
BEGIN
    TYPE NOTATION ::=
                  "LAST-UPDATED" value(Update ExtUTCTime)
                  "ORGANIZATION" Text
                  "CONTACT-INFO" Text
                  "DESCRIPTION" Text
                  RevisionPart

    VALUE NOTATION ::=
                  value(VALUE OBJECT IDENTIFIER)

    RevisionPart ::=
                  Revisions
                | empty
    Revisions ::=
                  Revision
                | Revisions Revision
    Revision ::=
                  "REVISION" value(Update ExtUTCTime)
                  "DESCRIPTION" Text

    -- a character string as defined in section 3.1.1
    Text ::= value(IA5String)
END

OBJECT-IDENTITY MACRO ::=
BEGIN
    TYPE NOTATION ::=
                  "STATUS" Status
                  "DESCRIPTION" Text

                  ReferPart

    VALUE NOTATION ::=
                  value(VALUE OBJECT IDENTIFIER)

    Status ::=
                  "current"
                | "deprecated"
                | "obsolete"

    ReferPart ::=
                  "REFERENCE" Text
                | empty

    -- a character string as defined in section 3.1.1
    Text ::= value(IA5String)
END

-- names of objects
-- (Note that these definitions of ObjectName and NotificationName
--  are not to be IMPORTed by MIB modules.)

ObjectName ::=
    OBJECT IDENTIFIER

NotificationName ::=
    OBJECT IDENTIFIER

-- syntax of objects

-- the "base types" defined here are:
--   3 built-in ASN.1 types: INTEGER, OCTET STRING, OBJECT IDENTIFIER
--   8 application-defined types: Integer32, IpAddress, Counter32,
--              Gauge32, Unsigned32, TimeTicks, Opaque, and Counter64

ObjectSyntax ::=
    CHOICE {
        simple
            SimpleSyntax,
          -- note that SEQUENCEs for conceptual tables and
          -- rows are not mentioned here...

        application-wide
            ApplicationSyntax
    }

-- built-in ASN.1 types

SimpleSyntax ::=
    CHOICE {
        -- INTEGERs with a more restrictive range
        -- may also be used
        integer-value               -- includes Integer32
            INTEGER (-2147483648..2147483647),
        -- OCTET STRINGs with a more restrictive size
        -- may also be used
        string-value
            OCTET STRING (SIZE (0..65535)),
        objectID-value
            OBJECT IDENTIFIER
    }

-- indistinguishable from INTEGER, but never needs more than
-- 32-bits for a two's complement representation
Integer32 ::=
        INTEGER (-2147483648..2147483647)

-- application-wide types

ApplicationSyntax ::=
    CHOICE {
        ipAddress-value
            IpAddress,
        counter-value
            Counter32,
        timeticks-value
            TimeTicks,
        arbitrary-value
            Opaque,
        big-counter-value
            Counter64,
        unsigned-integer-value  -- includes Gauge32
            Unsigned32
    }

-- in network-byte order

-- (this is a tagged type for historical reasons)
IpAddress ::=
    [APPLICATION 0]
        IMPLICIT OCTET STRING (SIZE (4))

-- this wraps
Counter32 ::=
    [APPLICATION 1]
        IMPLICIT INTEGER (0..4294967295)

-- this doesn't wrap
Gauge32 ::=
    [APPLICATION 2]
        IMPLICIT INTEGER (0..4294967295)

-- an unsigned 32-bit quantity
-- indistinguishable from Gauge32
Unsigned32 ::=
    [APPLICATION 2]
        IMPLICIT INTEGER (0..4294967295)

-- hundredths of seconds since an epoch
TimeTicks ::=
    [APPLICATION 3]
        IMPLICIT INTEGER (0..4294967295)

-- for backward-compatibility only
Opaque ::=
    [APPLICATION 4]
        IMPLICIT OCTET STRING

-- for counters that wrap in less than one hour with only 32 bits
Counter64 ::=
    [APPLICATION 6]
        IMPLICIT INTEGER (0..18446744073709551615)

-- definition for objects

OBJECT-TYPE MACRO ::=
BEGIN
    TYPE NOTATION ::=
                  "SYNTAX" Syntax
                  UnitsPart
                  "MAX-ACCESS" Access
                  "STATUS" Status
                  "DESCRIPTION" Text
                  ReferPart

                  IndexPart
                  DefValPart

    VALUE NOTATION ::=
                  value(VALUE ObjectName)

    Syntax ::=   -- Must be one of the following:
                       -- a base type (or its refinement),
                       -- a textual convention (or its refinement), or
                       -- a BITS pseudo-type
                   type
                | "BITS" "{" NamedBits "}"

    NamedBits ::= NamedBit
                | NamedBits "," NamedBit

    NamedBit ::=  identifier "(" number ")" -- number is nonnegative

    UnitsPart ::=
                  "UNITS" Text
                | empty

    Access ::=
                  "not-accessible"
                | "accessible-for-notify"
                | "read-only"
                | "read-write"
                | "read-create"

    Status ::=
                  "current"
                | "deprecated"
                | "obsolete"

    ReferPart ::=
                  "REFERENCE" Text
                | empty

    IndexPart ::=
                  "INDEX"    "{" IndexTypes "}"
                | "AUGMENTS" "{" Entry      "}"
                | empty
    IndexTypes ::=
                  IndexType
                | IndexTypes "," IndexType
    IndexType ::=
                  "IMPLIED" Index
                | Index

    Index ::=
                    -- use the SYNTAX value of the
                    -- correspondent OBJECT-TYPE invocation
                  value(ObjectName)
    Entry ::=
                    -- use the INDEX value of the
                    -- correspondent OBJECT-TYPE invocation
                  value(ObjectName)

    DefValPart ::= "DEFVAL" "{" Defvalue "}"
                | empty

    Defvalue ::=  -- must be valid for the type specified in
                  -- SYNTAX clause of same OBJECT-TYPE macro
                  value(ObjectSyntax)
                | "{" BitsValue "}"

    BitsValue ::= BitNames
                | empty

    BitNames ::=  BitName
                | BitNames "," BitName

    BitName ::= identifier

    -- a character string as defined in section 3.1.1
    Text ::= value(IA5String)
END

-- definitions for notifications

NOTIFICATION-TYPE MACRO ::=
BEGIN
    TYPE NOTATION ::=
                  ObjectsPart
                  "STATUS" Status
                  "DESCRIPTION" Text
                  ReferPart

    VALUE NOTATION ::=
                  value(VALUE NotificationName)

    ObjectsPart ::=
                  "OBJECTS" "{" Objects "}"
                | empty
    Objects ::=
                  Object

                | Objects "," Object
    Object ::=
                  value(ObjectName)

    Status ::=
                  "current"
                | "deprecated"
                | "obsolete"

    ReferPart ::=
                  "REFERENCE" Text
                | empty

    -- a character string as defined in section 3.1.1
    Text ::= value(IA5String)
END

-- definitions of administrative identifiers

zeroDotZero    OBJECT-IDENTITY
    STATUS     current
    DESCRIPTION
            "A value used for null identifiers."
    ::= { 0 0 }



TEXTUAL-CONVENTION MACRO ::=

BEGIN
    TYPE NOTATION ::=
                  DisplayPart
                  "STATUS" Status
                  "DESCRIPTION" Text
                  ReferPart
                  "SYNTAX" Syntax

    VALUE NOTATION ::=
                   value(VALUE Syntax)      -- adapted ASN.1

    DisplayPart ::=
                  "DISPLAY-HINT" Text
                | empty

    Status ::=
                  "current"
                | "deprecated"
                | "obsolete"

    ReferPart ::=
                  "REFERENCE" Text
                | empty

    -- a character string as defined in [2]
    Text ::= value(IA5String)

    Syntax ::=   -- Must be one of the following:
                       -- a base type (or its refinement), or
                       -- a BITS pseudo-type
                  type
                | "BITS" "{" NamedBits "}"

    NamedBits ::= NamedBit
                | NamedBits "," NamedBit

    NamedBit ::=  identifier "(" number ")" -- number is nonnegative

END

MODULE-COMPLIANCE MACRO ::=
BEGIN
    TYPE NOTATION ::=
                  "STATUS" Status
                  "DESCRIPTION" Text
                  ReferPart
                  ModulePart

    VALUE NOTATION ::=
                  value(VALUE OBJECT IDENTIFIER)

    Status ::=
                  "current"
                | "deprecated"
                | "obsolete"

    ReferPart ::=
                  "REFERENCE" Text
                | empty

    ModulePart ::=
                  Modules
    Modules ::=
                  Module
                | Modules Module
    Module ::=
                  -- name of module --
                  "MODULE" ModuleName
                  MandatoryPart
                  CompliancePart

    ModuleName ::=
                  -- identifier must start with uppercase letter
                  identifier ModuleIdentifier
                  -- must not be empty unless contained
                  -- in MIB Module
                | empty
    ModuleIdentifier ::=
                  value(OBJECT IDENTIFIER)
                | empty

    MandatoryPart ::=
                  "MANDATORY-GROUPS" "{" Groups "}"
                | empty

    Groups ::=

                  Group
                | Groups "," Group
    Group ::=
                  value(OBJECT IDENTIFIER)

    CompliancePart ::=
                  Compliances
                | empty

    Compliances ::=
                  Compliance
                | Compliances Compliance
    Compliance ::=
                  ComplianceGroup
                | Object

    ComplianceGroup ::=
                  "GROUP" value(OBJECT IDENTIFIER)
                  "DESCRIPTION" Text

    Object ::=
                  "OBJECT" value(ObjectName)
                  SyntaxPart
                  WriteSyntaxPart
                  AccessPart
                  "DESCRIPTION" Text

    -- must be a refinement for object's SYNTAX clause
    SyntaxPart ::= "SYNTAX" Syntax
                | empty

    -- must be a refinement for object's SYNTAX clause
    WriteSyntaxPart ::= "WRITE-SYNTAX" Syntax
                | empty

    Syntax ::=    -- Must be one of the following:
                       -- a base type (or its refinement),
                       -- a textual convention (or its refinement), or
                       -- a BITS pseudo-type
                  type
                | "BITS" "{" NamedBits "}"

    NamedBits ::= NamedBit
                | NamedBits "," NamedBit

    NamedBit ::= identifier "(" number ")" -- number is nonnegative

    AccessPart ::=
                  "MIN-ACCESS" Access
                | empty
    Access ::=
                  "not-accessible"
                | "accessible-for-notify"
                | "read-only"
                | "read-write"
                | "read-create"

    -- a character string as defined in [2]
    Text ::= value(IA5String)
END

OBJECT-GROUP MACRO ::=
BEGIN
    TYPE NOTATION ::=
                  ObjectsPart
                  "STATUS" Status
                  "DESCRIPTION" Text
                  ReferPart

    VALUE NOTATION ::=
                  value(VALUE OBJECT IDENTIFIER)

    ObjectsPart ::=
                  "OBJECTS" "{" Objects "}"
    Objects ::=
                  Object
                | Objects "," Object
    Object ::=

                  value(ObjectName)

    Status ::=
                  "current"
                | "deprecated"
                | "obsolete"

    ReferPart ::=
                  "REFERENCE" Text
                | empty

    -- a character string as defined in [2]
    Text ::= value(IA5String)
END

InterfaceIndex ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d"
    STATUS       current
    DESCRIPTION
            "A unique value, greater than zero, for each interface or
            interface sub-layer in the managed system.  It is
            recommended that values are assigned contiguously starting
            from 1.  The value for each interface sub-layer must remain
            constant at least from one re-initialization of the entity's
            network management system to the next re-initialization."
    SYNTAX       Integer32 (1..2147483647)



MacAddress ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "1x:"
    STATUS       current
    DESCRIPTION
            "Represents an 802 MAC address represented in the
            `canonical' order defined by IEEE 802.1a, i.e., as if it
            were transmitted least significant bit first, even though
            802.5 (in contrast to other 802.x protocols) requires MAC
            addresses to be transmitted most significant bit first."
    SYNTAX       OCTET STRING (SIZE (6))

END