NVME-ZNS-CLOSE-ZO(1)

NAME
nvme-zns-close-zone - Closes one or all zones

SYNOPSIS

nvme zns close-zone nvme zns id-ctrl <device> [--namespace-id=<NUM> | -n <NUM>]
                                                [--start-lba=<LBA> | -s <LBA>]
                                                [--select-all | -a]

DESCRIPTION

For the NVMe device given, issues the Zone Management Send command with the "Close Zone" action. This will transition the zone to the closed state.

The <device> parameter is mandatory and may be either the NVMe character device (ex: /dev/nvme0), or a namespace block device (ex: /dev/nvme0n1).

OPTIONS

-n <NUM>, --namespace-id=<NUM>
    Use the provided namespace id for the command. If not provided, the namespace id of the block device will be used. If the command is issued to a non-block device, the parameter is required.

-s <lba>, --start-lba=<lba>
    The starting LBA of the zone to close.

-a, --select-all
    Select all zones for this action

EXAMPLES

    • Close all zones on namespace 1:

        # nvme zns close-zone /dev/nvme0 -a -n 1

NVME

Part of nvme-cli