# nvme-lnvm-id-ns(1)

# nvme-lnvm-id-ns(1) Manual Page

## NAME

nvme-lnvm-id-ns - Identify Geometry for LightNVM NVMe device

## SYNOPSIS

    nvme lnvm-id-ns <device> [--namespace-id=<nsid> | -n <nsid>]
                            [--force | -f]
                            [--raw-binary | -b]
                            [--human-readable | -H]

## DESCRIPTION

Send an Identify Geometry command to the given LightNVM device, returns properties of the specified namespace in either human-readable or binary format.

## OPTIONS

--namespace-id=<nsid>
-n <nsid>

  Retrieve the geometry from the selected namespace.

--force
-f

  Try to read the data and assume it is a LightNVM device

--raw-binary
-b

  Output the raw output

--human-readable
-H

  Output the status in human readable format

## EXAMPLES

- Retrieve the geometry from nvme0

    # nvme lnvm-id-ns /dev/nvme0 -n 1

## NVME

Part of the nvme-user suite