nvme-fdp-events(1)
==================

NAME
----
nvme-fdp-events - Get Flexible Data Placement Events

SYNOPSIS
--------
[verse]
'nvme fdp events' <device> [--endgrp-id=<NUM> | -e <NUM>]
			   [--host-events | -E]
			   [--raw-binary | -b]
			   [--output-format=<FMT> | -o <FMT>]

DESCRIPTION
-----------
For the NVMe device given, provide information about events affecting Reclaim
Units and media usage in an Endurance Group.

OPTIONS
-------
-e <NUM>::
--endgrp-id=<NUM>::
	The endurance group identifier to use when requesting the log page.

-E::
--host-events::
	Request the controller to report host events.

-b::
--raw-binary::
	Print the raw buffer to the standard output stream.

-o <format>::
--output-format=<format>::
	Set the reporting format to 'normal', 'json', or 'binary'. Only one
	output format can be used at a time.

NVME
----
Part of nvme-cli
